IFC building model
Schema: "IFC2X3"
File name: "Sample.ifc"
Time stamp: "12/11/2021 2:47:11 PM"
Preprocessor: "IfcOpenShell 0.5.0-dev"
Originating system: "IfcOpenShell 0.5.0-dev"
Application: "Klemen" version "v1.0" by Organization (no name given)

People and organizations
  Person (no name given) of Organization (no name given)
  Owner history of Person (no name given) of Organization (no name given) | application "Klemen" version "v1.0" by Organization (no name given) | change ADDED | created 1636438754 (2021-11-09T06:19:14Z) | last modified by Person (no name given) of Organization (no name given) with "Klemen" version "v1.0" by Organization (no name given)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)

Spatial structure
IFCPROJECT "002610000"
  IFCSITE "Default Site"
    IFCBUILDING "Default Building"
      IFCBUILDINGSTOREY "Default Storey"
        contains 14 elements
          14 x IFCBUILDINGELEMENTPROXY | names: "Origin", "X_Axis", "Z_Axis" (+11 more) | property sets: Basic product data:, Dimensions:, Technical data:, Logistic data:, Manufacturer data:, Contacts:

Property sets
  Basic product data: | properties | on 14 objects (14 IFCBUILDINGELEMENTPROXY)
    Code: = "002610000" (IFCTEXT)
    Name: = "CH8x32 gG 1A/400V" (IFCTEXT)
    Product group: = "C - Low voltage cylindrical fuses" (IFCTEXT)
    Product link: = "https://www.etigroup.eu/products-services/002610000" (IFCTEXT)
    Short description: = "Fuse link, CH8x32 gG 1A/400V" (IFCTEXT)
  Dimensions: | properties | on 14 objects (14 IFCBUILDINGELEMENTPROXY)
    Depth (mm): = "8.5" (IFCTEXT)
    Height (mm): = "31.5" (IFCTEXT)
    Width (mm): = "8.5" (IFCTEXT)
  Technical data: | properties | on 14 objects (14 IFCBUILDINGELEMENTPROXY)
    Frequency (Hz): = "50" (IFCTEXT)
    Fusing characteristics: = "gG" (IFCTEXT)
    IP Rating: = "/" (IFCTEXT)
    Number of poles: = "/" (IFCTEXT)
    Power dissipation (W): = "2.5" (IFCTEXT)
    Rated current (A): = "1" (IFCTEXT)
    Rated voltage AC (V): = "400" (IFCTEXT)
    Rated voltage DC (V): = "/" (IFCTEXT)
    Voltage type: = "AC" (IFCTEXT)
    Weight (kg): = "0.004" (IFCTEXT)
  Logistic data: | properties | on 14 objects (14 IFCBUILDINGELEMENTPROXY)
    Basic packaging: = "10" (IFCTEXT)
    EAN (single product): = "38388951387601" (IFCTEXT)
  Manufacturer data: | properties | on 14 objects (14 IFCBUILDINGELEMENTPROXY)
    City: = "Izlake" (IFCTEXT)
    Country: = "Slovenia" (IFCTEXT)
    Manufacturer: = "ETI Elektroelement d.o.o." (IFCTEXT)
    Postal code: = "1411" (IFCTEXT)
    Street: = "Obrezija 5" (IFCTEXT)
    Website: = "https://www.etigroup.eu/" (IFCTEXT)
  Contacts: | properties | on 14 objects (14 IFCBUILDINGELEMENTPROXY)
    E-mail: = "support@eti.si" (IFCTEXT)
    Fax: = "00386 (0)3 / 56-74-077" (IFCTEXT)
    Telephone: = "00386 (0)3 / 56-57-570" (IFCTEXT)
  ETIM Classification v7.0: | properties | on 14 objects (14 IFCBUILDINGELEMENTPROXY)
    Breaking capacity (kA): = "50" (IFCTEXT)
    Class name: = "Cylindrical fuse" (IFCTEXT)
    Classification: = "EC002704" (IFCTEXT)
    Nominal current (A): = "1" (IFCTEXT)
    Size: = "Other" (IFCTEXT)
    Utilization category: = "Other" (IFCTEXT)